OziExplorer Map Data File Version 2.2
Lesne_cesty_sk-l7.tif [LC4]
C:\Users\Laco\Desktop\ogf2\LC4.png
1 ,Map Code,
WGS 84,WGS 84,   0.0000,   0.0000,WGS 84
Reserved 1
Reserved 2
Magnetic Variation,,,E
Map Projection,Lambert Conformal Conic,PolyCal,No,AutoCalOnly,No,BSBUseWPX,No
Point01,xy,    0,    0,in, deg,  48,51.92628,N,  18,52.23642,E, grid,   ,           ,           ,S
Point02,xy,18880,    0,in, deg,  48,56.41812,N,  20, 34.2207,E, grid,   ,           ,           ,S
Point03,xy,18880,14120,in, deg,  48,   6.093,N,  20, 38.4138,E, grid,   ,           ,           ,S
Point04,xy,    0,14120,in, deg,  48,   1.674,N,  18, 58.0872,E, grid,   ,           ,           ,S
Point05,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point06,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point07,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point08,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point09,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point10,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point11,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point12,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point13,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point14,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point15,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point16,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point17,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point18,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point19,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point20,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point21,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point22,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point23,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point24,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point25,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point26,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point27,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point28,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point29,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Point30,xy,     ,     ,in, deg,    ,        ,S,    ,        ,E, grid,   ,           ,           ,S
Projection Setup,    59.834920000,    24.833333000,,,,    47.605000000,    49.225000000,,,
Map Feature = MF ; Map Comment = MC     These follow if they exist
Track File = TF      These follow if they exist
Moving Map Parameters = MM?    These follow if they exist
MM0,Yes
MMPNUM,4
MMPXY,1,0,0
MMPXY,2,18880,0
MMPXY,3,18880,14120
MMPXY,4,0,14120
MMPLL,1,  18.870607,  48.865438
MMPLL,2,  20.570345,  48.940302
MMPLL,3,  20.640230,  48.101550
MMPLL,4,  18.968120,  48.027900
MM1B,6.604921
LL Grid Setup
LLGRID,No,No Grid,Yes,255,16711680,0,No Labels,0,16777215,7,1,Yes,x
Other Grid Setup
GRGRID,No,No Grid,Yes,255,16711680,No Labels,0,16777215,8,1,Yes,No,No,x
MOP,Map Open Position,0,0
IWH,Map Image Width/Height,18881,14121
